;****************************************************************************
;                                                                           *
;       Novell NetWare Server Driver Description File for RTGBSRV.LAN        *
;                                                                           *
;****************************************************************************

VER: 1.00
SYN: 1.00

DR RTGBSRV
{
    DES:    $RTGBSRV_1
    HELP:   $RTGBSRV_2
    PAR:    2.00
    PROD:   'PCI.10EC.8169.*.*.*',
            'PCI.10EC.8167.*.*.*'

;@# SPROD:  'TRENDnet, TEG-PCITXR  32-bit 10/100/1000Mbps PCI ADAPTER driver'
;@# ALIAS:  RTGBSRV.LAN
;@# CLIENT: RTGBSRV.LAN

    FILE:   RTGBSRV.LAN
    TIME:   15

    PR SLOT
    {
        DES:    $RTGBSRV_3
        HELP:   $RTGBSRV_4

        TYP:   DEC
        VAL:    1-65535
        DEF:    UND
        OUT:    'SLOT=%s'
    }

    FR FrameSelect
    {
        CD:     $RTGBSRV_5
        CH:     $RTGBSRV_6
        CD:     $RTGBSRV_7
        CH:     $RTGBSRV_8
        CD:     $RTGBSRV_9
        CH:     $RTGBSRV_10
        CD:     $RTGBSRV_11
        CH:     $RTGBSRV_12
        DEF:    1,2,3,4
    }

    PR NODE OPT
    {
        DES:    $RTGBSRV_13
        TYP:   HEX
        VAL:    1-FFFFFFFFFFFE
        DEF:    UND
        OUT:    'NODE=%s'
    }

}


DLANG:    4
;English
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    6
;French
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
                 expansion slot where the board is installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    7
;German
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board is installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    8
;Italian
    $RTGBSRV_1 = "TRENDnet, TEG-PCITXR  32-bit 10/100/1000Mbps PCI ADAPTER driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board is installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    14
;Spanish
    $RTGBSRV_1 = "TRENDnet, TEG-PCITXR  32-bit 10/100/1000Mbps PCI ADAPTER driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    12
;Portuquese
    $RTGBSRV_1 = "TRENDnet, TEG-PCITXR  32-bit 10/100/1000Mbps PCI ADAPTER driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    9
;Japanese
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    10
;Korean
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    1
;Chinese (Simplified)
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    16
;Chinese (Traditional)
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"

LANG:    13
;Russian
    $RTGBSRV_1 = "RTL8169 /8110 Family Gigabit Ethernet Network Adapter driver"
    $RTGBSRV_2 = "This driver supports PCI bus devices"
    $RTGBSRV_3 = "Slot"
    $RTGBSRV_4 = "Select the slot number that corresponds to the physical
            expansion slot where the board installed."
    $RTGBSRV_5 = "802.2"
    $RTGBSRV_6 = "ethernet_802.2"
    $RTGBSRV_7 = "802.3"
    $RTGBSRV_8 = "ethernet_802.3"
    $RTGBSRV_9 = "SNAP"
    $RTGBSRV_10 = "ethernet_snap"
    $RTGBSRV_11 = "ethernet II"
    $RTGBSRV_12 = "ethernet_II"
    $RTGBSRV_13 = "Node Address"
    $RTGBSRV_14 = "MediumType Select"
    $RTGBSRV_15 = "Support mediumtype keyword : AUTO, 100FULL, 100HALF, 10FULL, 10HALF"
