1. To build the driver open a terminal session and type "make clean" then 
   type "make" to create ft1000usb.ko device driver.
2. Create a folder /etc/flarion and copy ft3000.img to that directory.
3. Type the command insmod ./ft1000usb.ko to load the driver.
4. Plug in the Expresscard (or USB device) and wait couple seconds for the blue link led to blink.
Remark: Due to machine interop,if you meet problem when unplug and replug then you need to reload 
driver after unplug and replug. i.e. rmmod ./ft1000usb.ko and then insmod ./ft1000usb.ko
