;############################################################################       
;  Name:						rtgbsrv.111
;
;  Version:	  	  	V1.12
;
;  Released By:   	Russel Wang
;                 	
;  Release Date:  	03/03/08
;                 	
;  Changed File:  	rtgbsrv.c,rtgbsrv.def, rtgesrv.def rtesrv.def
;
;  Reason:	  	
;			1. Add support to RTL8102E(L)
;			2. MOdify Phy parameter for RTL8168C and RTL8168CP
;		
;  Comment:    
;	
;############################################################################       
;  Name:						rtgbsrv.111
;
;  Version:	  	  	V1.11
;
;  Released By:   	Russel Wang
;                 	
;  Release Date:  	08/13/07
;                 	
;  Changed File:  	rtgbsrv.c,rtgesrv.def,rtgesrv.ldi
;
;  Reason:	  	
			1. Add support to RTL8168CP
			2. Update RTL8168C Phy Parameter
;		
;  Comment:    
;	
;############################################################################         
;  Name:						rtgbsrv.110
;
;  Version:	  	  	V1.10
;
;  Released By:   	Russel Wang
;                 	
;  Release Date:  	04/16/07
;                 	
;  Changed File:  	rtgbsrv.c,rtgesrv.def,rtgesrv.ldi
;
;  Reason:	  	Add support to RTL8168C/8111C 
;		
;  Comment:    
;	
;############################################################################
;  Name:						rtgbsrv.109
;
;  Version:	  	  	V1.09
;
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	06/29/06
;                 	
;  Changed File:  	rtgbsrv.c,rtgbsrv.def,rtgesrv.def,rtgesrv.ldi,rtesrv.def,rtesrv.ldi
;
;  Reason:	  	  
;		
;  Comment:    
;				  					1. Modify PHY Parameters of RTL8169S
;										2. Fix multicat packet problem with chariot test
;										3. Adjust parameters with RTL8101E at initiale time
;
;############################################################################    
;  Name:			rtgbsrv.108
;
;  Version:	  	  	V1.08
;
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	02/21/06
;                 	
;  Changed File:  	rtgbsrv.c,rtgbsrv.def
;
;  Reason:	  	  
;		
;  Comment:    
;				  					1. Modify parameter with RTL8100E
;										2. Adjust PHY Parameters of RTL8169/RTL8168/RTl810XE series
;
;############################################################################    
;  Name:	  	  		rtgbsrv.107
;                 	
;  Version:	  	  	V1.07
;                 	
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	02/14/06
;                 	
;  Changed File:  	rtgbsrv.c
;
;  Reason:	  	  
;		
;  Comment:    
;				  		    	1. Support RTL8110SC that DID is "8167"
;             			2. Name of RTL8169 is "RTGBSRV",
;					   					 Name of RTL8168 is "RTGESRV",
;					   					 Name of RTL8100E/RTL8101E is "RTESRV",
;
;############################################################################  
;  Name:	  	  	rtesrv.106
;                 	
;  Version:	  	  	V1.06
;                 	
;  Released By:   	Vika Yen
;                 	
;  Release Date:  	12/09/05
;                 	
;  Changed File:  	rtesrv.c
;				  	rtesrv.def
;		  		  	rtesrv.ldi
;		  		  	rtesrv.txt
;
;  Reason:	  	  	Support RTL8169/8168B/810XE serial Novell Server Driver
;		          	
;  Comment:       	
;				  	  1.Support NW4.X/5.X/6.X
;		  		  	2.Support RTL8169SC 
;		  		  	3.Support RTL8101E
;		  		  	4.Set MWIEN be 0 with RTL8169SC
;		  		  	5.Adjust RTL8168/810XE multicast order
;		  		  	6.RCB with 8-byte aligment
;				  	  7.Resolve to install EMM386 with client32
;                 
;
;############################################################################        
;  Name:	  		rtesrv.105
;             		
;  Version:	  		V1.05
;               	
;  Released By: 	Vika Yen
;               	
;  Release Date:	08/03/05
;               	
;  Changed File:	rtesrv.c
;		  			rtesrv.def
;		  			rtesrv.ldi
;		  			rtesrv.txt
;               	
;  Reason:	  		Release RTL8168B Novell Server Driver
;		        	
;  Comment:     	
;		  			1. Set Priority queue polling level, when ISR is TOK and TDU.
;		  			2. set ETThR be 0x27 (0xEC,0x27)
;		  			3. Rx Flow Control be disable.
;		  			4. Set RTL8168B Phy paraemeter  			 
;		  			5. max DMA Burst Size=512   
;                 
;############################################################################        
;  Name:	  		rtgbsrv.104
;
;  Version:	  		V1.04
;
;  Released By:   	ken
;
;  Release Date:  	10/30/03
;
;  Changed File:  	rtgbsrv
;
;  Reason:	  		modify the PHY parameter for the .13C
;		
;  Comment:       
;                 
;################################################################################
;  Name:	 	 	rtgbsrv.103
;
;  Version:	  		V1.03
;
;  Released By:   	ken
;
;  Release Date:  	10/30/03
;
;  Changed File:  	rtgbsrv
;
;  Reason:	  		modify the PHY parameter for the .13B
;		
;  Comment:       
;                 
;################################################################################        
;  Name:	  		rtgbsrv.102
;
;  Version:	  		V1.02
;
;  Released By:   	ken
;
;  Release Date:  	10/30/03
;
;  Changed File:  	rtgbsrv
;
;  Reason:	  		check the PHY version (0 or 1)
;		
;  Comment:       
;                 
;################################################################################        
;  Name:	  		rtgbsrv.101
;
;  Version:	  		V1.01
;
;  Released By:   	ken
;
;  Release Date:  	6/27/03
;
;  Changed File:  	rtgbsrv.c
;
;  Reason:	  		Add the PHY parameter for the 8110
;		
;  Comment:       
;                 
;
;################################################################################
;
;
;  Name:	  		rtgbsrv.100
;
;  Version:	  		V1.00
;
;  Released By:   	ken
;
;  Release Date:  	6/12/02
;
;  Changed File:  	rtgbsrv.c
;
;  Reason:	  
;		
;  Comment:       
;                 
;################################################################################
