NetWare DOS ODI Driver Installation

Use the Novell DOS ODI client driver(RTGEODI.COM) to connect to an existing Novell Server.

Connect to a Server and install drivers:

1.  Prepare these files:  

    LSL.COM
    RTGEODI.COM
    IPXODI.COM
    VLM.COM

2. Modify parameter such as link speed, frame type, etc in NET.CFG file.

3. At the DOS prompt, load these files in the following order:

    LSL
    RTGEODI
    IPXODI
    VLM


Disconnect from a Server and unload drivers: 

At DOS prompt, unload these files in the following order:
  
    VLM U  
    IPXODI U 
    RTGEODI U
    LSL U


 

