2006/04/07
version:v1.30
FreeBSD driver support RTL8169SC/8110SC

2006/04/10
version:v1.40
FreeBSD driver support RTL8168B/8111B

2006/04/11
version:v1.50
FreeBSD driver support RTL8101E

2006/04/12
version:v1.60
FreeBSD driver support RTL8160SB/8110SB

2006/05/10
version:v1.70
FreeBSD 5.4/6.0 driver support RTL8169S/8110S, RTK8169SB/8110SB, RTL8110SC, RTL8168B/8111B, and RTL8101E.

2006/08/18
version:v1.71
1. modify the phy parameter
2. support promiscuous mode
3. process interrupts in a finite loop

2006/10/20
version:v1.72
implement the interrupt handler of rx fifo overflow

2007/04/17
version:v1.73
Support RTL8168C/8111C

2007/08/20
version:v1.74
Turn on phy when driver is loaded.

2008/01/08
version:v1.75
1. Support RTL8102E/8102EL 
2. Support RTL8111CP 
3. Edit the E-PHY and G-PHY parameters of RTL8111C 
4. Edit GPHY parameters of RTL8110SC 
5. Read MAC address from MAC registers
6. In Readme, correct the command for forcing to half duplex
