                           TEW-658BRM Release Note 

Notes: 
Upgraded Firmware will not do factory reset, please make sure to save your settings. 
User needs to do factory reset once the firmware upgrade procedure is completed and then upload saved settings.

Default settings:
Default IP 		: 192.168.10.1
Default Login		: admin/admin



Firmware Version: v1.03.B06
Date: 02/14/2013



Notes: 
Updated UPnP protection to address vulnerability issues. 
Improve wireless stability


___________________________________________________________________________________________________________________


Firmware Version: v1.03.B04
Date: 08/30/2012


Notes: 
Added IPv6 support
Allow MRU 1500 can be set on UI when PPPoA/PPPoE mode.

___________________________________________________________________________________________________________________



Firmware Version: v1.02.B18
Date: 03/28/2012


Notes: 
WPA encryption allows special characters
Improve URL filter
Changeable passphrase with WPA/WPA2-TKIP/AES in MBSSID
GUI updates
___________________________________________________________________________________________________________________


Firmware Version: v1.02.B14
Date: 07/27/2011

Notes: 
Allow one character PPPoE passwords
Fixed Windows 7 wireless client will never prompt for WPS message when connecting

___________________________________________________________________________________________________________________


Firmware Version: v1.02.B12
Date: 07/27/2011

Notes: 
Update DSL auto scan list
Set PPPoE passthrough default value to disable
Automatically set DUT MAC ID When PPPoE passthrough is enabled


___________________________________________________________________________________________________________________

Firmware Version: v1.02.B10	

Notes:
-Enahnced DSL auto scan wizard
-Set connection trigger to "Always On"

___________________________________________________________________________________________________________________

Firmware: 1.02.B08

Notes: 
Initial release

