File name: Firmware_TS-U100_1.98.ZIP
Date: March-1-2006

Description:
Firmware file: TS-U100_1.98.bin 
Date: Feb-15-2006.
TS-U100 - USB 2.0 Network Storage Server Firmware version 1.98

========================================
Release Note
========================================

Firmware version 1.98
1. Fixed "Linux command can access Storage Server" issue.
2. Fixed "directory/folder path not display correctly" when using FireFox Browser.

Previous firmware version 1.86 Date: Mar-25-2005

========================================
Warning! 
========================================

Firmware upgrade failure may permanently damage the unit, causing it to malfunction.
If the issues in the “Release Note” do not address the problem you are experiencing with the TS-U100,
please do not upgrade the firmware.

DO NOT perform the upgrade via a wireless connection.

Please also manually record the TS-U100's configuration settings, in case the unit loses the settings after the firmware upgrade.

========================================
Disclaimer
========================================

Our advice is strictly limited to the questions asked and is based on the information provided
to us. TRENDnet does not assume any responsibility or liability for the advice given and shall
not be liable for any direct, indirect, special, incidental or consequential damages in connection
with the use of this information. Always back up your data. For more information, including
technical information updates, please visit our Web site at www.trendnet.com.


========================================
 Firmware Upgrade Procedures
========================================

1. Please download, save, and unzip the new firmware file (record the file path) to a network Computer’s hard drive.

2. Network this Computer (using a network cable) to the TS-U100 (Network Storage Server) and 
configure this Computer’s TCP/IP settings for accessing TS-U100's configuration page. You can network the Computer directly to 
TS-U100's LAN port or connect them to a network Hub, Switch or Router's LAN port (make sure no other network devices are using 
the same IP addresses). After powering on these equipments, check the TS-U100’s front panel, make sure the “Power” LED light
 is solid green and the “LAN” LED light is solid green.

3. Close all running programs on the Computer that you will use to perform the firmware upgrade.

4. From the Computer, open a web browser (e.g. Internet Explorer), and open the TS-U100’s configuration page
 (default address: http://192.168.1.2). At the login window, type in the "username" and “password” 
(default username: admin, password: admin), and click “ok”.

5. On the “Advanced” page, under “status”, look for “Firmware Version”. If it is "1.98.0215.2006" or newer, please do not perform
the firmware upgrade. Otherwise, click on "maintenance" on the menu option, under “Firmware Upload”, type in the
new firmware file path (from Step 1 above) or click on “Browse”, locate and open the new firmware file “TS-U100_1.98.bin”, 
and then click on “Upload”.

6. Confirm the firmware file name and file path on the screen and click “OK” to start the upgrade.
<<Warning!>> DO NOT interrupt the upgrade progress. During the upgrade process, DO NOT disconnect the network cable and power adapter, 
DO NOT press the reset button, DO NOT power off the TS-U100, and DO NOT power off the Computer.

7. When you see the firmware upgrade successful message on the screen, click the "Restart" button to restart the unit. 
Once restarted it will return you to the login screen. Wait 30 seconds for the TS-U100 to reboot, then type username and
password (Same as Step 4) to configure your unit. If you do not see the Information page on the screen, close the web browser,
reboot the computer, open the web browser and then open the TS-U100's configuration page (default: http://192.168.1.2).

8. Click “Advanced” on the menu bar, click "Status", then look for the “Firmware version”. If it shows “1.98.0215.2006), the upgrade is successful.

========================================
 Technical Support
========================================

If you need assistance performing the firmware upgrade or if you have any questions, please contact our Technical Support Team.

The Tech Support Hours are Mon. ~ Fri., 7:00AM ~ 6:00PM, 
Pacific Standard Time 
(except major holidays).

Tel:  310-626-6252
Fax: 310-626-6267
E-mail: support@trendnet.com
www.trendnet.com

European Support Center
Tech Support Hours
8:00am - 6:00pm 
Middle European Time 
Monday - Friday

Telephone
Deutsch : +49 (0) 6331 / 268-460 
Français: +49 (0) 6331 / 268-461
	: 0800-907-161 (numéro vert)  
Español : +49 (0) 6331 / 268-462 
Eesti   : +372-6593613 (9.00AM to 5:00PM)  
English : +49 (0) 6331 / 268-463  
Italiano: +49 (0) 6331 / 268-464 
Dutch:  : +49 (0) 6331 / 268-465 

Fax
+49 (0) 6331 / 268-466 

========================================
   Thank you for choosing TRENDnet.
========================================